
****



始于心，终于心 www.horrol.com


专业电子生产设备制造商 / Professional electronic production equipment manufacturer


**半自动锡膏印刷机**

**Semi automatic solder paste printing machine**

此设备应用于SMT生产线电路板的刮锡膏操作

This equipment is used for scraping solder paste in SMT production line

半自动锡膏印刷机特点：1、蜂窝平台定位2、双片悬浮刮刀3、三位一体电磁阀控制4、X、Y轴旋钮微调5、PLC集成控制6、真彩屏简易操作页面Features of Semi automatic solder paste printing machine:1. Positioning of cellular platform2. Double suspension scraper3. Three in one solenoid valve control4. Fine adjustment of x-axis and y-axis knobs­­­5. PLC integrated control6. Simple operation page of true color screen



**半自动锡膏印刷机技术规格参数 / Technical specification parameters of semi-automatic solder paste printing machine**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 设备型号Equipment model | HR-SAPP-400 | HR-SAPP-600 | HR-SAPP-1200 | HR-SAPP-1500 |
| 外形尺寸Boundary dimension | 700x900x1680mm | 900x900x1680mm | 1500x900x1680mm | 1800x900x1680mm |
| 工作台板Worktable board | 500x320mm | 700x320mm | 1300x320mm | 1600x320mm |
| 钢网允许尺寸Steel mesh size | 600x450mm | 800x450mm | 1400x450mm | 1700x450mm |
| 控制模块Control module | PLC 工控 | PLC工控 | PLC工控 | PLC工控 |
| 触摸彩屏Touch color screen | 4.3寸/inch Kineal | 4.3寸/inch Kineal | 4.3寸/inch Kineal | 4.3寸/inch Kineal |
| 主动气缸Main cylinder | SC63x150-S | SC63x150-S | SC63x150-S | SC63x150-S |
| 刀头气缸Cutter head cylinder | CDU25x50 | CDU25x50 | CDU25x50 | CDU25x50 |
| 滑动导轨Slide guide | 直线导轨linear guide rail | 直线导轨linear guide rail | 直线导轨linear guide rail | 直线导轨linear guide rail |
| 变频器Frequency converter | ENC | ENC | ENC | ENC |
| 印刷精度Printing accuracy | ±0.02mm | ±0.02mm | ±0.02mm | ±0.02mm |
| 微调范围Fine tuning range | ±10mm | ±10mm | ±10mm | ±10mm |
| 移动电机Mobile motor | 三相/60w Three phase / 60W | 三相/60w Three phase / 60W | 三相/60w Three phase / 60W | 三相/60w Three phase / 60W |
| 电源电压Supply voltage | 单相/220v Single phase / 220 V | 单相220v Single phase / 220 V | 单相220v Single phase / 220 V | 单相220v Single phase / 220 V |
| 启动功率Starting power | 0.2kw | 0.2kw | 0.2kw | 0.2kw |
| 气源Air source | 0.5Mpa-0.8Mpa | 0.5Mpa-0.8Mpa | 0.5Mpa-0.8Mpa | 0.5Mpa-0.8Mpa |
| 移动方向Direction of movement | 左右可移Left and right movable | 左右可移Left and right movable | 左右可移Left and right movable | 左右可移Left and right movable |
| 移动速度Movement speed | 0~2200mm/min | 0~2200mm/min | 0~2200mm/min | 0~2200mm/min |
| 设备重量Equipment weight | 195kg | 245kg | 280kg | 340kg |

上述产品由广东海森堡科技有限公司及广东合瑞科技有限公司设计、生产